Back To Index << Back To Templates

# Template Boundary Observation

Aus Publikation für Projekt ELGA Basisleitfäden | Release 11.12.0+20260729-2.6.6 vom 2026‑07‑29 08:38:14 | | | HTML erstellt am 2026‑07‑29 09:00:25

Id | 2.16.840.1.113883.10.20.6.2.11 | Gültigkeit ab | 2015‑08‑13
Status | Entwurf | Versions-Label | 2.1
Name | BoundaryObservation | Bezeichnung | Boundary Observation
Beschreibung
A Boundary Observation contains a list of integer values for the referenced frames of a DICOM multiframe image SOP instance. It identifies the frame numbers within the referenced SOP instance to which the reference applies. The CDA Boundary Observation numbers frames using the same convention as DICOM, with the first frame in the referenced object being Frame 1. A Boundary Observation must be used if a referenced DICOM SOP instance is a multiframe image and the reference does not apply to all frames.
Kontext | Elternknoten des Template-Element mit Id 2.16.840.1.113883.10.20.6.2.11
Klassifikation | CDA Entry Level Template
Offen/Geschlossen | Offen (auch andere als die definierten Elemente sind erlaubt)
Benutzt von / Benutzt |
Benutzt von 1 Transaction und 6 Templates, Benutzt 0 Templates
Benutzt von | als | Name | Version
--- | --- | --- | ---
elga-transactions-98 | Transaktion | Befund Bildgebende Diagnostik (v2) | 2023‑05‑09 07:19:00
2.16.840.1.113883.10.20.6.2.10 | Containment | Referenced Frames Observation (2.1) | 2015‑08‑13
2.16.840.1.113883.10.20.6.2.8 |  | SOP Instance Observation (2.1) | 2015‑08‑13
2.16.840.1.113883.10.20.22.4.63 |  | Series Act (2.1) | 2015‑08‑13
2.16.840.1.113883.10.20.6.2.6 |  | Study Act (2.1) | 2015‑08‑13
2.16.840.1.113883.10.20.6.1.1 |  | DICOM Object Catalog Section - DCM 121181 (2.1) | 2015‑08‑13
1.2.40.0.34.11.5 |  | Befund Bildgebende Diagnostik | 2023‑04‑17 12:20:09
Beziehung | Spezialisierung: Template 2.16.840.1.113883.10.12.303 CDA Observation (2005‑09‑07) ref ad1bbr-
Item | DT | Kard | Konf | Beschreibung | Label
--- | --- | --- | --- | --- | ---
cda:observation |  |  |  |  |
@classCode |  | 1 … 1 | F | OBS | CONF9282
| SHALL contain exactly one [1..1] @classCode="OBS" Observation (CodeSystem: HL7ActClass urn:oid:2.16.840.1.113883.5.6 STATIC) (CONF:81-9282).
@moodCode |  | 1 … 1 | F | EVN | CONF9283
| SHALL contain exactly one [1..1] @moodCode="EVN" Event (CodeSystem: HL7ActClass urn:oid:2.16.840.1.113883.5.6 STATIC) (CONF:81-9283).
cda:templateId | II | 1 … 1 | M | Note: this element was not in the C-CDA 2.1 specification but was present in the example and is normally present on every observation template. Considered this to be an inconsistency in the specification. |
@root |  | 1 … 1 | F | 2.16.840.1.113883.10.20.6.2.11
cda:code | CD | 1 … 1 | M | SHALL contain exactly one [1..1] code (CONF:81-9284). | CONF9284
@code | CONF | 1 … 1 | F | 113036
@codeSystem | 1 … 1 | F | 1.2.840.10008.2.16.4 (DCM)
cda:value | INT | 1 … * | R | SHALL contain at least one [1..*] value with @xsi:type="INT" (CONF:81-9285). Each number represents a frame for display. | CONF9285