Back To Index << Back To Templates

# Template SOP Instance Observation

Aus Publikation für Projekt ELGA Basisleitfäden | Release 11.12.0+20260729-2.6.6 vom 2026‑07‑29 08:38:14 | | | HTML erstellt am 2026‑07‑29 09:00:25

Id | 2.16.840.1.113883.10.20.6.2.8 | Gültigkeit ab | 2015‑08‑13
Status | Entwurf | Versions-Label | 2.1
Name | SOPInstanceObservation | Bezeichnung | SOP Instance Observation
Beschreibung
A SOP Instance Observation contains the DICOM Service Object Pair (SOP) Instance information for referenced DICOM composite objects. The SOP Instance act class is used to reference both image and non-image DICOM instances. The text attribute contains the DICOM WADO reference.
Kontext | Elternknoten des Template-Element mit Id 2.16.840.1.113883.10.20.6.2.8
Klassifikation | CDA Entry Level Template
Offen/Geschlossen | Offen (auch andere als die definierten Elemente sind erlaubt)
Benutzt von / Benutzt |
Benutzt von 1 Transaction und 4 Templates, Benutzt 2 Templates
Benutzt von | als | Name | Version
--- | --- | --- | ---
elga-transactions-98 | Transaktion | Befund Bildgebende Diagnostik (v2) | 2023‑05‑09 07:19:00
2.16.840.1.113883.10.20.22.4.63 | Containment | Series Act (2.1) | 2015‑08‑13
2.16.840.1.113883.10.20.6.2.6 |  | Study Act (2.1) | 2015‑08‑13
2.16.840.1.113883.10.20.6.1.1 |  | DICOM Object Catalog Section - DCM 121181 (2.1) | 2015‑08‑13
1.2.40.0.34.11.5 |  | Befund Bildgebende Diagnostik | 2023‑04‑17 12:20:09
Benutzt | als | Name | Version
2.16.840.1.113883.10.20.6.2.9 | Containment | Purpose of Reference Observation (2.1) | 2015‑08‑13
2.16.840.1.113883.10.20.6.2.10 | Containment | Referenced Frames Observation (2.1) | 2015‑08‑13
Beziehung | Spezialisierung: Template 2.16.840.1.113883.10.12.303 CDA Observation (2005‑09‑07) ref ad1bbr-
Item | DT | Kard | Konf | Beschreibung | Label
--- | --- | --- | --- | --- | ---
cda:observation |  |  |  |  |
wo [cda:code/@codeSystem='1.2.840.10008.2.6.1'] |
@classCode |  | 1 … 1 | F | DGIMG | CONF9240
| SHALL contain exactly one [1..1] @classCode="DGIMG" Diagnostic Image (CodeSystem: HL7ActClass urn:oid:2.16.840.1.113883.5.6 STATIC) (CONF:81-9240).
@moodCode |  | 1 … 1 | F | EVN | CONF9241
| SHALL contain exactly one [1..1] @moodCode="EVN" Event (CodeSystem: ActMood urn:oid:2.16.840.1.113883.5.1001 STATIC) (CONF:81-9241).
cda:templateId | II | 1 … 1 | M | Note: this element was not in the C-CDA 2.1 specification but was present in the example and is normally present on every observation template. Considered this to be an inconsistency in the specification. |
@root |  | 1 … 1 | F | 2.16.840.1.113883.10.20.6.2.8
cda:id | II | 1 … * |  | SHALL contain at least one [1..*] id (CONF:81-9242). The @root contains an OID representing the DICOM SOP Instance UID | CONF9242
cda:code |  | 1 … 1 | M | SHALL contain exactly one [1..1] code (CONF:81-9244). a. This code SHALL contain exactly one [1..1] @code (CONF:81-19225). i. @code is an OID for a valid SOP class name UID (CONF:81-19226). b. This code SHALL contain exactly one [1..1] @codeSystem="1.2.840.10008.2.6.1" DCMUID (CONF:81-19227). | CONF9244
@codeSystem | CONF | 1 … 1 | F | 1.2.840.10008.2.6.1 (DICOM UID)
cda:text |  | 0 … 1 | R | SHOULD contain zero or one [0..1] text (CONF:81-9246). | CONF9246
@mediaType |  | 1 … 1 | F | application/dicom | CONF9247
| The text, if present, SHALL contain exactly one [1..1] @mediaType="application/dicom" (CONF:81-9247).
cda:reference |  | 1 … 1 |  | The text, if present, SHALL contain exactly one [1..1] reference (CONF:81-9248). | CONF9248
| Constraint | SHALL contain a @value that contains a WADO reference as a URI
cda:effectiveTime |  | 0 … 1 | R | SHOULD contain zero or one [0..1] effectiveTime (CONF:81-9250). | CONF9250
@value |  | 1 … 1 | R | The effectiveTime, if present, SHALL contain exactly one [1..1] @value (CONF:81-9251). | CONF9251
cda:low |  |  | NP |  | CONF9252
| Constraint | The effectiveTime, if present, SHALL NOT contain [0..0] low (CONF:81-9252).
cda:high |  |  | NP |  | CONF9253
| Constraint | The effectiveTime, if present, SHALL NOT contain [0..0] high (CONF:81-9253).
cda:entryRelationship |  | 0 … * |  | MAY contain zero or more [0..*] entryRelationship (CONF:81-9254) such that it | CONF9254
@typeCode |  | 1 … 1 | F | SUBJ | CONF9255
| SHALL contain exactly one [1..1] @typeCode="SUBJ" Has Subject (CodeSystem: HL7ActRelationshipType urn:oid:2.16.840.1.113883.5.1002 STATIC) (CONF:81-9255).
cda:entryRelationship |  | 0 … * |  | Beinhaltet 2.16.840.1.113883.10.20.6.2.9 Purpose of Reference Observation (2015‑08‑13) | CONF9257
@typeCode |  | 1 … 1 | F | RSON | CONF9258
| SHALL contain exactly one [1..1] @typeCode="RSON" Has Reason (CodeSystem: HL7ActRelationshipType urn:oid:2.16.840.1.113883.5.1002 STATIC) (CONF:81-9258).
cda:entryRelationship |  | 0 … * |  | Beinhaltet 2.16.840.1.113883.10.20.6.2.10 Referenced Frames Observation (2015‑08‑13) | CONF9260
@typeCode |  | 1 … 1 | F | COMP | CONF9261
| SHALL contain exactly one [1..1] @typeCode="COMP" Has Component (CodeSystem: HL7ActRelationshipType urn:oid:2.16.840.1.113883.5.1002 STATIC) (CONF:81-9261).
| Constraint | This entryRelationship SHALL be present if the referenced DICOM object is a multiframe object and the reference does not apply to all frames